1.	NJM3548 and NJM3545 are obsolete with no direct replacement. Require re-design with new style High and Low Side Drivers. Replace with Infineon drivers (specifications in documentation folder).
2.